{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["废水比对","废水排放"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水比对","index":0,"n_rows":11,"n_cols":14,"rows_kept":11,"merged":[[1,0,10,0],[1,1,5,1],[6,1,10,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","样品类型","手动监测值","自动监测值","比对结果","技术要求"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表1）传染病、结核病医疗机构水污染物排放限值在（日均值）,采用其他消毒方式","污水排放口","pH值","2024-08-01","实际样","7.2","7.2","0pH","绝对误差不超过±0.5pH"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","化学需氧量","2024-08-01","实际样","50","51","2%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","化学需氧量","2024-08-01","实际样","48","51","6.25%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","化学需氧量","2024-08-01","实际样","50","47","-6%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","化学需氧量","2024-08-01","标准样","250","265","6%","相对误差不超过±10%"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","化学需氧量","2024-08-01","实际样","37","29","-21.62%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","化学需氧量","2024-08-01","实际样","37","28","-24.32%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","化学需氧量","2024-08-01","实际样","38","28","-26.32%","相对误差不超过±30%"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","化学需氧量","2024-08-01","标准样","239","250","4.6%","相对误差不超过±10%"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","医疗机构水污染物排放标准(GB18466-2005)","（表1）传染病、结核病医疗机构水污染物排放限值在（日均值）,采用其他消毒方式","污水排放口DW001","pH值","2024-08-01","实际样","7.3","7.2","-0.1pH","绝对误差不超过±0.5pH"]

{"sheet":"废水排放","index":1,"n_rows":41,"n_cols":22,"rows_kept":41,"merged":[[1,0,30,0],[1,1,15,1],[16,1,20,1],[21,1,30,1],[31,0,40,0],[31,1,35,1],[36,1,40,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","受纳水体","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","生产负荷(%)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排口DW001(01)","悬浮物","2024-07-25","","27.6","","","17","400","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排口DW001(01)","动植物油","2024-07-25","","27.6","","","0.22","100","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排口DW001(01)","pH值","2024-07-25","","27.6","","","7.2","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排口DW001(01)","化学需氧量","2024-07-25","","27.6","","","22","500","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排口DW001(01)","石油类","2024-07-25","","27.6","","","0.38","20","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW003(03)","pH值","2024-07-25","","29.9","","","7.8","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW003(03)","化学需氧量","2024-07-25","","29.9","","","12","500","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW003(03)","动植物油","2024-07-25","","29.9","","","0.22","100","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW003(03)","悬浮物","2024-07-25","","29.9","","","15","400","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW003(03)","石油类","2024-07-25","","29.9","","","0.38","20","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW002(02)","化学需氧量","2024-07-25","","27.8","","","21","500","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW002(02)","悬浮物","2024-07-25","","27.8","","","15","400","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002(02)","石油类","2024-07-25","","27.8","","","0.52","20","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002(02)","动植物油","2024-07-25","","27.8","","","0.19","100","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","南京汽轮电机（集团）有限责任公司","水环境,大气环境","汽轮机及辅机制造","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002(02)","pH值","2024-07-25","","27.8","","","7.4","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","江苏金陵环境股份有限公司城北污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口DW001(DW001)","pH值","2024-07-25","","28.7","","","6.9","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","江苏金陵环境股份有限公司城北污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口DW001(DW001)","悬浮物","2024-07-25","","28.7","","","6","10","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","江苏金陵环境股份有限公司城北污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口DW001(DW001)","化学需氧量","2024-07-25","","28.7","","","5","50","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","江苏金陵环境股份有限公司城北污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口DW001(DW001)","动植物油","2024-07-25","","28.7","","","0.19","1","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","江苏金陵环境股份有限公司城北污水处理厂","水环境","污水处理及其再生利用","","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口DW001(DW001)","石油类","2024-07-25","","28.7","","","0.52","1","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002","石油类","2024-07-23","","27.1","","","1.34","20","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW002","化学需氧量","2024-07-23","","27.1","","","16","500","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002","pH值","2024-07-23","","27.1","","","7.8","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW002","动植物油","2024-07-23","","27.1","","","0.90","100","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW002","悬浮物","2024-07-23","","27.1","","","16","400","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW001","悬浮物","2024-07-23","","27.6","","","55","400","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,其他排污单位,三级标准","污水排放口DW001","化学需氧量","2024-07-23","","27.6","","","106","500","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW001","pH值","2024-07-23","","27.6","","","7.5","9","6","无量纲","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW001","动植物油","2024-07-23","","27.6","","","0.14","100","","mg/L","否","","","是"]
["招商局金陵船舶（南京）有限公司等3家企业","招商局金陵船舶（南京）有限公司","水环境,大气环境","铁路、船舶、航空航天和其他运输设备制造业","","污水综合排放标准(GB8978-1996)","（表4）第二类污染物最高允许排放浓度（1998年1月1日后建的单位）,一切排污单位 ,三级标准","污水排放口DW001","石油类","2024-07-23","","27.6","","","0.32","20","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","悬浮物","2024-08-01","","30.3","","","45","60","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表1）传染病、结核病医疗机构水污染物排放限值在（日均值）,采用其他消毒方式","污水排放口","pH值","2024-08-01","","30.3","","","7.2","9","6","无量纲","否","","","是"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","化学需氧量","2024-08-01","","30.3","","","49","250","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","动植物油","2024-08-01","","30.3","","","0.35","20","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京脑科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口","石油类","2024-08-01","","30.3","","","0.37","20","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","动植物油","2024-08-01","","30.2","","","0.17","20","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","化学需氧量","2024-08-01","","30.2","","","37","250","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表1）传染病、结核病医疗机构水污染物排放限值在（日均值）,采用其他消毒方式","污水排放口DW001","pH值","2024-08-01","","30.2","","","7.3","9","6","无量纲","否","","","是"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","污水排放口DW001","悬浮物","2024-08-01","","30.2","","","27","60","","mg/L","否","","","是"]
["南京脑科医院、南京胸科医院","南京市胸科医院","水环境","医院","","医疗机构水污染物排放标准(GB18466-2005)","（表1）传染病、结核病医疗机构水污染物排放限值在（日均值）,采用其他消毒方式","污水排放口DW001","石油类","2024-08-01","","30.2","","","0.27","20","","mg/L","否","","","是"]